[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=10 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=10 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18114 FreeMB:29982 SharedMB:952 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000388028 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0003882e8 FreeGB:0xc0003882f0} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0003882f8 FreeGB:0xc000388330}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000300588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:1a:ce:e1:14:eb:42 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:48004.89 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:38.75 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:49.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:42.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18114 FreeMB:29982 SharedMB:952 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000388028 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0003882e8 FreeGB:0xc0003882f0} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0003882f8 FreeGB:0xc000388330}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000300588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:1a:ce:e1:14:eb:42 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:48004.89 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:38.75 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:49.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:42.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    79%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:37302.325 EventsPerSecSingle:5589.62 EventsPerSecMulti:69015.03 DurationSec:20.0005 Score:37302.325 ScoreSingle:5589.62 ScoreMulti:69015.03}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8164.38 Score:8164.38}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=917.19 MB/s read=14453.27 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768167139295274745.fio]
[DEBUG] [3/6] Bench disque final -> read=14453.27 MB/s write=917.19 MB/s score=7685.23
[DEBUG] [3/6] Résultat disque: {ReadMBs:14453.26551746065 WriteMBs:917.1936277176725 IOPSRead:9535.482151 IOPSWrite:9539.215359 LatencyMs:0.081910128785 Score:7685.229572589161}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:940.2466482896066 Download:938.0459117868456 PingMs:0.242 JitterMs:<nil> PacketLossPct:<nil> Score:939.1462800382261}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:37302.325 EventsPerSecSingle:5589.62 EventsPerSecMulti:69015.03 DurationSec:20.0005 Score:37302.325 ScoreSingle:5589.62 ScoreMulti:69015.03} Memory:{Throughput:8164.38 Score:8164.38} Disk:{ReadMBs:14453.26551746065 WriteMBs:917.1936277176725 IOPSRead:9535.482151 IOPSWrite:9539.215359 LatencyMs:0.081910128785 Score:7685.229572589161} Network:{Upload:940.2466482896066 Download:938.0459117868456 PingMs:0.242 JitterMs:<nil> PacketLossPct:<nil> Score:939.1462800382261} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1865.12 mem=81.64 disk=768.52 net=93.91
[DEBUG] Score global calculé : 92547.13
[DEBUG] Payload JSON (49197 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.951,
      "max_freq_ghz": 4.951,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18114,
      "free_mb": 29982,
      "shared_mb": 952,
      "slots_total": 10,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 34
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.3539276123047,
          "free_gb": 61.39210510253906
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "1a:ce:e1:14:eb:42",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 48004.89,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 33.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 38.75,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 49.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 42.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 33.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    79%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 37302.325,
      "events_per_sec_single": 5589.62,
      "events_per_sec_multi": 69015.03,
      "duration_s": 20.0005,
      "score": 37302.325,
      "score_single": 5589.62,
      "score_multi": 69015.03
    },
    "memory": {
      "throughput_mib_s": 8164.38,
      "score": 8164.38
    },
    "disk": {
      "read_mb_s": 14453.26551746065,
      "write_mb_s": 917.1936277176725,
      "iops_read": 9535.482151,
      "iops_write": 9539.215359,
      "latency_ms": 0.081910128785,
      "score": 7685.229572589161
    },
    "network": {
      "upload_mbps": 940.2466482896066,
      "download_mbps": 938.0459117868456,
      "ping_ms": 0.242,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 939.1462800382261
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 92547.13142521653
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    79%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49197 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=10 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=10 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18275 FreeMB:29821 SharedMB:979 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc00011a030 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00011a2f0 FreeGB:0xc00011a2f8} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00011a330 FreeGB:0xc00011a338}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000388588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:52:56:ee:7b:ba:d3 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49148.4 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:45.75 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:39 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18275 FreeMB:29821 SharedMB:979 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc00011a030 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00011a2f0 FreeGB:0xc00011a2f8} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00011a330 FreeGB:0xc00011a338}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000388588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:52:56:ee:7b:ba:d3 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49148.4 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:45.75 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:39 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    81%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:36969.91 EventsPerSecSingle:5587.94 EventsPerSecMulti:68351.88 DurationSec:20.0004 Score:36969.91 ScoreSingle:5587.94 ScoreMulti:68351.88}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8347.92 Score:8347.92}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=915.05 MB/s read=14375.91 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768168282802413389.fio]
[DEBUG] [3/6] Bench disque final -> read=14375.91 MB/s write=915.05 MB/s score=7645.48
[DEBUG] [3/6] Résultat disque: {ReadMBs:14375.906463009333 WriteMBs:915.0527733432826 IOPSRead:9828.939035 IOPSWrite:9828.539049 LatencyMs:0.07898161341000001 Score:7645.479618176308}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:941.609346041091 Download:938.5134446046105 PingMs:0.289 JitterMs:<nil> PacketLossPct:<nil> Score:940.0613953228508}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:36969.91 EventsPerSecSingle:5587.94 EventsPerSecMulti:68351.88 DurationSec:20.0004 Score:36969.91 ScoreSingle:5587.94 ScoreMulti:68351.88} Memory:{Throughput:8347.92 Score:8347.92} Disk:{ReadMBs:14375.906463009333 WriteMBs:915.0527733432826 IOPSRead:9828.939035 IOPSWrite:9828.539049 LatencyMs:0.07898161341000001 Score:7645.479618176308} Network:{Upload:941.609346041091 Download:938.5134446046105 PingMs:0.289 JitterMs:<nil> PacketLossPct:<nil> Score:940.0613953228508} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1848.50 mem=83.48 disk=764.55 net=94.01
[DEBUG] Score global calculé : 91840.42
[DEBUG] Payload JSON (49197 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.951,
      "max_freq_ghz": 4.951,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18275,
      "free_mb": 29821,
      "shared_mb": 979,
      "slots_total": 10,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 33
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.3690605163574,
          "free_gb": 61.37697219848633
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "52:56:ee:7b:ba:d3",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 49148.4,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 32.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 45.75,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 39,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 28.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 32.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    81%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 36969.91,
      "events_per_sec_single": 5587.94,
      "events_per_sec_multi": 68351.88,
      "duration_s": 20.0004,
      "score": 36969.91,
      "score_single": 5587.94,
      "score_multi": 68351.88
    },
    "memory": {
      "throughput_mib_s": 8347.92,
      "score": 8347.92
    },
    "disk": {
      "read_mb_s": 14375.906463009333,
      "write_mb_s": 915.0527733432826,
      "iops_read": 9828.939035,
      "iops_write": 9828.539049,
      "latency_ms": 0.07898161341000001,
      "score": 7645.479618176308
    },
    "network": {
      "upload_mbps": 941.609346041091,
      "download_mbps": 938.5134446046105,
      "ping_ms": 0.289,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 940.0613953228508
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 91840.42463167547
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    81%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49197 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0xA (10)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=10 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=10 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18475 FreeMB:29621 SharedMB:979 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d14a0 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0002d1760 FreeGB:0xc0002d1768} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0002d17a0 FreeGB:0xc0002d17a8}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc0005aec38 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0a:56:a4:c0:d5:6c IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49397.39 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:37.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:42 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:29.25 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18475 FreeMB:29621 SharedMB:979 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d14a0 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0002d1760 FreeGB:0xc0002d1768} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0002d17a0 FreeGB:0xc0002d17a8}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc0005aec38 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0a:56:a4:c0:d5:6c IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49397.39 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:37.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:42 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:29.25 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    76%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:37366.34 EventsPerSecSingle:5594.59 EventsPerSecMulti:69138.09 DurationSec:20.0004 Score:37366.34 ScoreSingle:5594.59 ScoreMulti:69138.09}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8873.54 Score:8873.54}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=896.99 MB/s read=16272.41 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768168531800702966.fio]
[DEBUG] [3/6] Bench disque final -> read=16272.41 MB/s write=896.99 MB/s score=8584.70
[DEBUG] [3/6] Résultat disque: {ReadMBs:16272.405274777706 WriteMBs:896.9909953233824 IOPSRead:3638.945368 IOPSWrite:3628.379054 LatencyMs:0.244814307753 Score:8584.698135050545}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:941.2978240228581 Download:938.859237154658 PingMs:0.197 JitterMs:<nil> PacketLossPct:<nil> Score:940.078530588758}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:37366.34 EventsPerSecSingle:5594.59 EventsPerSecMulti:69138.09 DurationSec:20.0004 Score:37366.34 ScoreSingle:5594.59 ScoreMulti:69138.09} Memory:{Throughput:8873.54 Score:8873.54} Disk:{ReadMBs:16272.405274777706 WriteMBs:896.9909953233824 IOPSRead:3638.945368 IOPSWrite:3628.379054 LatencyMs:0.244814307753 Score:8584.698135050545} Network:{Upload:941.2978240228581 Download:938.859237154658 PingMs:0.197 JitterMs:<nil> PacketLossPct:<nil> Score:940.078530588758} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1868.32 mem=88.74 disk=858.47 net=94.01
[DEBUG] Score global calculé : 94616.86
[DEBUG] Payload JSON (49196 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.951,
      "max_freq_ghz": 4.951,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18475,
      "free_mb": 29621,
      "shared_mb": 979,
      "slots_total": 10,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 33
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.37024307250977,
          "free_gb": 61.375789642333984
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "0a:56:a4:c0:d5:6c",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 49397.39,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 32.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 37.625,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 42,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 29.25,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 32.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 37366.34,
      "events_per_sec_single": 5594.59,
      "events_per_sec_multi": 69138.09,
      "duration_s": 20.0004,
      "score": 37366.34,
      "score_single": 5594.59,
      "score_multi": 69138.09
    },
    "memory": {
      "throughput_mib_s": 8873.54,
      "score": 8873.54
    },
    "disk": {
      "read_mb_s": 16272.405274777706,
      "write_mb_s": 896.9909953233824,
      "iops_read": 3638.945368,
      "iops_write": 3628.379054,
      "latency_ms": 0.244814307753,
      "score": 8584.698135050545
    },
    "network": {
      "upload_mbps": 941.2978240228581,
      "download_mbps": 938.859237154658,
      "ping_ms": 0.197,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 940.078530588758
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 94616.86280068984
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49196 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0xA (10)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=10 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=10 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18708 FreeMB:29388 SharedMB:973 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000388038 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0003882f8 FreeGB:0xc000388300} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000388308 FreeGB:0xc000388340}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000012ae8 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:c2:20:55:8b:9c:ff IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49830.32 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:49.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:38.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28.25 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18708 FreeMB:29388 SharedMB:973 SlotsTotal:10 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000388038 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0003882f8 FreeGB:0xc000388300} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000388308 FreeGB:0xc000388340}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000012ae8 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:c2:20:55:8b:9c:ff IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:49830.32 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:49.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:38.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28.25 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    82%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:36977.61 EventsPerSecSingle:5605.24 EventsPerSecMulti:68349.98 DurationSec:20.0004 Score:36977.61 ScoreSingle:5605.24 ScoreMulti:68349.98}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8845.03 Score:8845.03}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=920.69 MB/s read=13922.23 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768168964714568679.fio]
[DEBUG] [3/6] Bench disque final -> read=13922.23 MB/s write=920.69 MB/s score=7421.46
[DEBUG] [3/6] Résultat disque: {ReadMBs:13922.228872774444 WriteMBs:920.69257516124 IOPSRead:9534.715509 IOPSWrite:9537.915403 LatencyMs:0.08189057620500001 Score:7421.460723967842}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:942.760280024577 Download:939.5252128746424 PingMs:0.239 JitterMs:<nil> PacketLossPct:<nil> Score:941.1427464496097}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:36977.61 EventsPerSecSingle:5605.24 EventsPerSecMulti:68349.98 DurationSec:20.0004 Score:36977.61 ScoreSingle:5605.24 ScoreMulti:68349.98} Memory:{Throughput:8845.03 Score:8845.03} Disk:{ReadMBs:13922.228872774444 WriteMBs:920.69257516124 IOPSRead:9534.715509 IOPSWrite:9537.915403 LatencyMs:0.08189057620500001 Score:7421.460723967842} Network:{Upload:942.760280024577 Download:939.5252128746424 PingMs:0.239 JitterMs:<nil> PacketLossPct:<nil> Score:941.1427464496097} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1848.88 mem=88.45 disk=742.15 net=94.11
[DEBUG] Score global calculé : 91508.29
[DEBUG] Payload JSON (49200 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.951,
      "max_freq_ghz": 4.951,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18708,
      "free_mb": 29388,
      "shared_mb": 973,
      "slots_total": 10,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 34
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.3708190917969,
          "free_gb": 61.375213623046875
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "c2:20:55:8b:9c:ff",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 49830.32,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 33.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 49.125,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 38.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 28.25,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 33.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    82%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 36977.61,
      "events_per_sec_single": 5605.24,
      "events_per_sec_multi": 68349.98,
      "duration_s": 20.0004,
      "score": 36977.61,
      "score_single": 5605.24,
      "score_multi": 68349.98
    },
    "memory": {
      "throughput_mib_s": 8845.03,
      "score": 8845.03
    },
    "disk": {
      "read_mb_s": 13922.228872774444,
      "write_mb_s": 920.69257516124,
      "iops_read": 9534.715509,
      "iops_write": 9537.915403,
      "latency_ms": 0.08189057620500001,
      "score": 7421.460723967842
    },
    "network": {
      "upload_mbps": 942.760280024577,
      "download_mbps": 939.5252128746424,
      "ping_ms": 0.239,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 941.1427464496097
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 91508.2901943853
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    82%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49200 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0x4 (4)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=4 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=4 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18641 FreeMB:29455 SharedMB:988 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00043a078 FreeGB:0xc00043a080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00043a088 FreeGB:0xc00043a0c0}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc00043a548 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0e:6b:00:3b:c5:a6 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50280.49 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:40.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:41.75 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18641 FreeMB:29455 SharedMB:988 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00043a078 FreeGB:0xc00043a080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00043a088 FreeGB:0xc00043a0c0}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc00043a548 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0e:6b:00:3b:c5:a6 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50280.49 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:40.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:41.75 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    71%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0x4 (4)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=4 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=4 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18643 FreeMB:29452 SharedMB:988 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc000436078 FreeGB:0xc000436080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000436088 FreeGB:0xc0004360c0}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000481098 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0e:6b:00:3b:c5:a6 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50293.2 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:55.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:38.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:27.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.951 MaxFreqGHz:4.951 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18643 FreeMB:29452 SharedMB:988 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc000436078 FreeGB:0xc000436080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000436088 FreeGB:0xc0004360c0}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000481098 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:0e:6b:00:3b:c5:a6 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50293.2 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:55.625 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:38.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:27.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    76%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:36751.07 EventsPerSecSingle:5595.73 EventsPerSecMulti:67906.41 DurationSec:20.0004 Score:36751.07 ScoreSingle:5595.73 ScoreMulti:67906.41}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8832.02 Score:8832.02}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=901.92 MB/s read=15786.26 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768169427605069173.fio]
[DEBUG] [3/6] Bench disque final -> read=15786.26 MB/s write=901.92 MB/s score=8344.09
[DEBUG] [3/6] Résultat disque: {ReadMBs:15786.264489614423 WriteMBs:901.9169959817839 IOPSRead:9303.189894 IOPSWrite:9312.28959 LatencyMs:0.08482241337799999 Score:8344.090742798104}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:942.3453311386673 Download:939.4684180124369 PingMs:0.383 JitterMs:<nil> PacketLossPct:<nil> Score:940.9068745755521}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:36751.07 EventsPerSecSingle:5595.73 EventsPerSecMulti:67906.41 DurationSec:20.0004 Score:36751.07 ScoreSingle:5595.73 ScoreMulti:67906.41} Memory:{Throughput:8832.02 Score:8832.02} Disk:{ReadMBs:15786.264489614423 WriteMBs:901.9169959817839 IOPSRead:9303.189894 IOPSWrite:9312.28959 LatencyMs:0.08482241337799999 Score:8344.090742798104} Network:{Upload:942.3453311386673 Download:939.4684180124369 PingMs:0.383 JitterMs:<nil> PacketLossPct:<nil> Score:940.9068745755521} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1837.55 mem=88.32 disk=834.41 net=94.09
[DEBUG] Score global calculé : 92897.63
[DEBUG] Payload JSON (49197 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.951,
      "max_freq_ghz": 4.951,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18643,
      "free_mb": 29452,
      "shared_mb": 988,
      "slots_total": 4,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 33
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.37347412109375,
          "free_gb": 61.37255859375
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "0e:6b:00:3b:c5:a6",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 50293.2,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 32.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 55.625,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 38.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 27.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 32.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 36751.07,
      "events_per_sec_single": 5595.73,
      "events_per_sec_multi": 67906.41,
      "duration_s": 20.0004,
      "score": 36751.07,
      "score_single": 5595.73,
      "score_multi": 67906.41
    },
    "memory": {
      "throughput_mib_s": 8832.02,
      "score": 8832.02
    },
    "disk": {
      "read_mb_s": 15786.264489614423,
      "write_mb_s": 901.9169959817839,
      "iops_read": 9303.189894,
      "iops_write": 9312.28959,
      "latency_ms": 0.08482241337799999,
      "score": 8344.090742798104
    },
    "network": {
      "upload_mbps": 942.3453311386673,
      "download_mbps": 939.4684180124369,
      "ping_ms": 0.383,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 940.9068745755521
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 92897.63236017177
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49197 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0x4 (4)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=4 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=4 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18178 FreeMB:29918 SharedMB:966 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000400028 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0004002e8 FreeGB:0xc0004002f0} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0004002f8 FreeGB:0xc000400330}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000572ee8 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:72:1e:69:40:ac:37 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50783.82 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:51.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:31 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18178 FreeMB:29918 SharedMB:966 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc000400028 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:33} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc0004002e8 FreeGB:0xc0004002f0} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc0004002f8 FreeGB:0xc000400330}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000572ee8 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:72:1e:69:40:ac:37 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:50783.82 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:32.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:51.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:31 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:28 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:32.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    77%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:37224.47 EventsPerSecSingle:5584.58 EventsPerSecMulti:68864.36 DurationSec:20 Score:37224.47 ScoreSingle:5584.58 ScoreMulti:68864.36}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8835.26 Score:8835.26}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=899.14 MB/s read=15351.86 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768169918234495427.fio]
[DEBUG] [3/6] Bench disque final -> read=15351.86 MB/s write=899.14 MB/s score=8125.50
[DEBUG] [3/6] Résultat disque: {ReadMBs:15351.86 WriteMBs:899.14 IOPSRead:9350.72 IOPSWrite:9358.05 LatencyMs:0.08 Score:8125.5}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:942.45 Download:939.54 PingMs:0.3 JitterMs:<nil> PacketLossPct:<nil> Score:941}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:37224.47 EventsPerSecSingle:5584.58 EventsPerSecMulti:68864.36 DurationSec:20 Score:37224.47 ScoreSingle:5584.58 ScoreMulti:68864.36} Memory:{Throughput:8835.26 Score:8835.26} Disk:{ReadMBs:15351.86 WriteMBs:899.14 IOPSRead:9350.72 IOPSWrite:9358.05 LatencyMs:0.08 Score:8125.5} Network:{Upload:942.45 Download:939.54 PingMs:0.3 JitterMs:<nil> PacketLossPct:<nil> Score:941} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1861.22 mem=88.35 disk=812.55 net=94.10
[DEBUG] Score global calculé : 93407.99
[DEBUG] Payload JSON (49089 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.95,
      "max_freq_ghz": 4.95,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18178,
      "free_mb": 29918,
      "shared_mb": 966,
      "slots_total": 4,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 33
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.37604904174805,
          "free_gb": 61.3699836730957
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "72:1e:69:40:ac:37",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 50783.82,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 32.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 51.125,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 31,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 28,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 32.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    77%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 37224.47,
      "events_per_sec_single": 5584.58,
      "events_per_sec_multi": 68864.36,
      "duration_s": 20,
      "score": 37224.47,
      "score_single": 5584.58,
      "score_multi": 68864.36
    },
    "memory": {
      "throughput_mib_s": 8835.26,
      "score": 8835.26
    },
    "disk": {
      "read_mb_s": 15351.86,
      "write_mb_s": 899.14,
      "iops_read": 9350.72,
      "iops_write": 9358.05,
      "latency_ms": 0.08,
      "score": 8125.5
    },
    "network": {
      "upload_mbps": 942.45,
      "download_mbps": 939.54,
      "ping_ms": 0.3,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 941
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 93407.992
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    77%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49089 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0x4 (4)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=4 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=4 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18364 FreeMB:29732 SharedMB:991 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc000436078 FreeGB:0xc000436080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000436088 FreeGB:0xc0004360c0}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000300588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:ba:c8:d3:a7:be:c8 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:51348.21 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:53.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:40.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:29 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18364 FreeMB:29732 SharedMB:991 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc0002d1db8 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc000436078 FreeGB:0xc000436080} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc000436088 FreeGB:0xc0004360c0}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc000300588 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:ba:c8:d3:a7:be:c8 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:51348.21 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:53.125 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:40.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:29 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 0/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    76%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:37292.03 EventsPerSecSingle:5549.97 EventsPerSecMulti:69034.08 DurationSec:20 Score:37292.03 ScoreSingle:5549.97 ScoreMulti:69034.08}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8776.09 Score:8776.09}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=888.51 MB/s read=14874.14 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768170482660233585.fio]
[DEBUG] [3/6] Bench disque final -> read=14874.14 MB/s write=888.51 MB/s score=7881.33
[DEBUG] [3/6] Résultat disque: {ReadMBs:14874.14 WriteMBs:888.51 IOPSRead:10243.96 IOPSWrite:10239.03 LatencyMs:0.07 Score:7881.33}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:942.03 Download:939.3 PingMs:0.18 JitterMs:<nil> PacketLossPct:<nil> Score:940.67}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:37292.03 EventsPerSecSingle:5549.97 EventsPerSecMulti:69034.08 DurationSec:20 Score:37292.03 ScoreSingle:5549.97 ScoreMulti:69034.08} Memory:{Throughput:8776.09 Score:8776.09} Disk:{ReadMBs:14874.14 WriteMBs:888.51 IOPSRead:10243.96 IOPSWrite:10239.03 LatencyMs:0.07 Score:7881.33} Network:{Upload:942.03 Download:939.3 PingMs:0.18 JitterMs:<nil> PacketLossPct:<nil> Score:940.67} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1864.60 mem=87.76 disk=788.13 net=94.07
[DEBUG] Score global calculé : 93042.60
[DEBUG] Payload JSON (49106 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.95,
      "max_freq_ghz": 4.95,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18364,
      "free_mb": 29732,
      "shared_mb": 991,
      "slots_total": 4,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 34
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.38393783569336,
          "free_gb": 61.36209487915039
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "ba:c8:d3:a7:be:c8",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 51348.21,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 33.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 53.125,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 40.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 29,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 33.85,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 0/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 37292.03,
      "events_per_sec_single": 5549.97,
      "events_per_sec_multi": 69034.08,
      "duration_s": 20,
      "score": 37292.03,
      "score_single": 5549.97,
      "score_multi": 69034.08
    },
    "memory": {
      "throughput_mib_s": 8776.09,
      "score": 8776.09
    },
    "disk": {
      "read_mb_s": 14874.14,
      "write_mb_s": 888.51,
      "iops_read": 10243.96,
      "iops_write": 10239.03,
      "latency_ms": 0.07,
      "score": 7881.33
    },
    "network": {
      "upload_mbps": 942.03,
      "download_mbps": 939.3,
      "ping_ms": 0.18,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 940.67
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 93042.59800000003
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    76%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49106 octets)
[DEBUG] Contenu de /home/gilles/Documents/vscode/bis/bench_go/config.yaml :
# bench-client config.yaml
# Objectif: décrire précisément
# - les outils à utiliser (et exigences d'installation)
# - les informations à collecter
# - les benchmarks à exécuter
# - les paramètres (timeouts, limites, endpoints, debug)
#
# Le binaire (Go/Rust) charge ce fichier depuis HTTP(S), valide les bornes, applique des defaults sûrs,
# et peut fallback sur une config locale si indisponible.

config_version: 1
profile: default

backend:
  # URL finale du POST (le programme peut aussi accepter server_base_url + path)
  url: "http://10.0.0.50:8007/api/benchmark"
  # Auth: idéalement injecté par variable d'env sur le client; éviter de mettre le token dans la config distante.
  auth:
    mode: bearer_env
    env_var: "test_hardware_perf"
  http:
    timeout_s: 15
    retries: 2
    retry_backoff_s: 2
    tls:
      verify: true

remote_config:
  # Options de cache/ETag si le binaire gère le rafraîchissement
  cache_path: "/var/cache/bench-client/config.yaml"
  use_etag: true
  refresh_max_age_s: 86400

runtime:
  # Timeouts globaux de sécurité
  max_total_runtime_s: 480
  command_timeout_s: 30
  command_timeout_overrides:
    dmidecode_s: 20
    smartctl_s: 10
    lsblk_s: 10
    sysbench_cpu_s: 120
    sysbench_mem_s: 60
    fio_s: 120
    iperf3_s: 20
  temp_dir: "/tmp"
  locale: "C"
  path_prepend:
    - "/usr/sbin"
    - "/sbin"

logging:
  level: info          # trace|debug|info|warn|error
  progress: true       # affichage étapes (1/N) + items
  show_command_lines: false
  capture_raw_output: true   # remonte dans raw_info (attention taille)
  raw_output_max_kb: 5120
  save_payload_to_tmp: true
  payload_tmp_dir: "/tmp"
  payload_filename_prefix: "bench_payload_"
  interactive_pause_on_debug: true

payload:
  dir: "."
  prefix: "bench_payload_"
  always_save: true

device_identity:
  # device_identifier envoyé au backend
  prefer:
    - hostname
    - machine_id
  hostname_command: "hostname"
  machine_id_path: "/etc/machine-id"

dependencies:
  # Liste des programmes externes (installés par le script shell)
  # Le binaire doit pouvoir:
  # - détecter présence/version (optionnel)
  # - marquer chaque "feature" comme disponible ou non
  required_base:
    - name: "curl"
      purpose: "Téléchargements/diagnostics (souvent côté script)"
    - name: "jq"
      purpose: "Optionnel: debug/validation (souvent côté script, pas nécessaire au binaire)"
    - name: "lscpu"
      purpose: "Infos CPU"
    - name: "free"
      purpose: "Infos mémoire"
    - name: "lsblk"
      purpose: "Infos stockage/partitions"
    - name: "ip"
      purpose: "Interfaces réseau, adresses IP"
    - name: "bc"
      purpose: "Optionnel: calculs (si pas fait en code)"
    - name: "dmidecode"
      purpose: "Infos BIOS/carte mère/RAM/DMI"
      requires_root: true
    - name: "smartctl"
      package: "smartmontools"
      purpose: "Infos disques SMART"
      requires_root: true
    - name: "ethtool"
      purpose: "Vitesse réseau, Wake-on-LAN, driver"
      requires_root: true
    - name: "lspci"
      package: "pciutils"
      purpose: "Liste périphériques PCI (GPU/Audio/etc.)"
    - name: "lsusb"
      package: "usbutils"
      purpose: "Liste périphériques USB"
    - name: "aplay"
      package: "alsa-utils"
      purpose: "Inventaire audio ALSA"
    - name: "arecord"
      package: "alsa-utils"
      purpose: "Inventaire capture ALSA"
    - name: "pactl"
      package: "pulseaudio-utils"
      purpose: "Infos audio PulseAudio/PipeWire (si dispo)"
    - name: "iw"
      package: "iw"
      purpose: "SSID + bitrate Wi-Fi"
    - name: "loginctl"
      package: "systemd"
      purpose: "Type de session (x11/wayland/tty)"
    - name: "xrandr"
      package: "x11-xserver-utils"
      purpose: "Résolution écran (X11)"
    - name: "xdpyinfo"
      package: "x11-utils"
      purpose: "Résolution écran (fallback X11)"
    - name: "swaymsg"
      package: "sway"
      purpose: "Résolution écran (Wayland/Sway)"
    - name: "nvidia-smi"
      package: "nvidia-utils"
      purpose: "Infos GPU NVIDIA (si présent)"
    - name: "systemd-detect-virt"
      package: "systemd"
      purpose: "Détection virtualisation/proxmox"
    - name: "pveversion"
      package: "pve-manager"
      purpose: "Détection hôte Proxmox (si présent)"
  benchmark_tools:
    - name: "sysbench"
      purpose: "Bench CPU et mémoire"
    - name: "fio"
      purpose: "Bench disque"
    - name: "iperf3"
      purpose: "Bench réseau"
    - name: "ping"
      package: "iputils-ping"
      purpose: "Vérifier accessibilité iperf server"
    - name: "nc"
      package: "netcat-openbsd"
      purpose: "Tester port 5201 iperf3"

collection:
  # Liste des infos à récupérer, structurées comme dans ton script.
  system:
    enabled: true
    items:
      - hostname
      - os_id
      - os_version
      - kernel_version
      - architecture
      - session_type           # XDG_SESSION_TYPE / loginctl / DISPLAY / WAYLAND_DISPLAY
      - screen_resolution      # xrandr/xdpyinfo/swaymsg
      - last_boot_time         # who -b
      - uptime_seconds         # /proc/uptime
      - battery_percentage     # /sys/class/power_supply/BAT*/capacity
      - battery_status         # /sys/class/power_supply/BAT*/status
      - battery_health         # /sys/class/power_supply/BAT*/health ou uevent
      - virtualization         # systemd-detect-virt + proxmox hints
    virtualization_detection:
      enabled: true
      proxmox:
        detect_host_by:
          - pveversion
          - "/etc/pve"
        detect_guest_by:
          - systemd_detect_virt
          - qemu_guest_agent
          - dmidecode_manufacturer_product_matches: ["qemu", "proxmox"]
      capture:
        - is_proxmox_host
        - is_proxmox_guest
        - proxmox_version
        - virtualization_type

  cpu:
    enabled: true
    source:
      primary: lscpu
      supplement_dmidecode: true
    items:
      - vendor
      - model
      - cores_physical        # cores_per_socket * sockets
      - threads               # nproc
      - base_freq_ghz         # lscpu CPU MHz -> GHz
      - max_freq_ghz          # lscpu CPU max MHz -> GHz
      - cache_l1_kb
      - cache_l2_kb
      - cache_l3_kb
      - flags                 # CPU flags list
      - microarchitecture     # depuis dmidecode type 4 (Family) si manquant
    raw_capture:
      - lscpu_output

  ram:
    enabled: true
    sources:
      - free
      - dmidecode
    items:
      - total_mb
      - used_mb
      - free_mb
      - shared_mb
      - slots_total           # dmidecode -t 16
      - slots_used            # dmidecode -t 17
      - max_capacity_mb       # dmidecode -t 16 Maximum Capacity
      - ecc                   # dmidecode -t memory Error Correction Type
      - layout                # par slot: locator, size, type, speed, configured_speed, form_factor, type_detail, rank, manufacturer, part_number
    raw_capture:
      - dmidecode_full

  gpu:
    enabled: true
    sources:
      - lspci
      - nvidia_smi_optional
    items:
      - vendor                # NVIDIA/AMD/Intel/Unknown
      - model                 # lspci vga/3d ou nvidia-smi name
      - memory_dedicated_mb   # nvidia-smi (si dispo)
      - driver_version        # nvidia-smi (si dispo)

  motherboard_bios:
    enabled: true
    source: dmidecode
    items:
      - baseboard_manufacturer
      - baseboard_product_name
      - bios_vendor
      - bios_version
      - bios_release_date

  pci_devices:
    enabled: true
    source: lspci
    items:
      - slot
      - class
      - vendor
      - device

  usb_devices:
    enabled: true
    source: lsusb
    items:
      - bus
      - device
      - vendor_id
      - product_id
      - name

  audio:
    enabled: true
    sources:
      - lspci
      - alsa
      - pactl_optional
    items:
      hardware:
        - pci_audio_devices     # lspci audio
        - alsa_playback         # aplay -l
        - alsa_capture          # arecord -l
        - pcm_devices           # aplay -L
      software:
        - backend               # pipewire/pulseaudio/alsa
        - server_name
        - server_version
        - default_sink
        - default_source
        - sinks
        - sources

  storage:
    enabled: true
    sources:
      - lsblk
      - smartctl
    devices:
      enumerate_by: "lsblk_disks"   # lsblk -d -n -o NAME,TYPE
      include_removable: false
      items:
        - device                 # /dev/sda
        - model                  # smartctl -i
        - serial                 # smartctl -i
        - size                   # lsblk
        - type                   # rota -> ssd/hdd
        - interface              # tran
        - temperature_c          # smartctl -A
        - smart_health           # smartctl -H
    partitions:
      enabled: true
      source: lsblk_json
      items:
        - name
        - mount_point
        - fs_type
        - total_gb
        - used_gb
        - free_gb
    raw_capture:
      - lsblk_output

  network_shares:
    enabled: true
    source: "/proc/mounts"
    detect_fs_types:
      - nfs
      - nfs4
      - cifs
      - smbfs
      - fuse.cifs
      - fuse.smbfs
      - afp
      - afpfs
      - fuse.afpfs
      - sshfs
      - fuse.sshfs
      - ftpfs
      - curlftpfs
      - fuse.ftpfs
      - davfs
      - davfs2
      - fuse.webdavfs
    items:
      - protocol
      - source
      - mount_point
      - fs_type
      - options
      - total_gb
      - used_gb
      - free_gb

  network:
    enabled: true
    sources:
      - ip
      - ethtool
      - iw_optional
    interface_filter:
      # reprise logique script: UP|UNKNOWN sauf interfaces virtuelles connues
      include_states: ["UP", "UNKNOWN"]
      exclude_name_prefixes: ["lo", "docker", "br-", "veth", "tap", "fw"]
    items:
      - name
      - type                  # bridge|ethernet|wifi|unknown
      - mac
      - ip_address
      - speed_mbps            # ethtool speed ou iw tx bitrate
      - driver                # ethtool -i ou /sys/.../driver
      - ssid                  # iw dev link
      - wake_on_lan           # ethtool Wake-on

raw_info:
  enabled: true
  include:
    - lscpu
    - lsblk
    - dmidecode
  max_size_kb: 5120

benchmarks:
  enabled: true
  # Pondérations identiques à ton script (si résultat dispo)
  weights:
    cpu: 0.40
    memory: 0.20
    disk: 0.20
    network: 0.10
    gpu: 0.10

  cpu_sysbench:
    enabled: true
    tool: sysbench
    params:
      cpu_max_prime: 20000
      single_thread: 1
      multi_threads: "all"      # all -> nproc
    outputs:
      - events_per_sec_single
      - events_per_sec_multi
      - duration_s
      - score_single
      - score_multi
      - score_global

  memory_sysbench:
    enabled: true
    tool: sysbench
    params:
      total_size: "1G"
    outputs:
      - throughput_mib_s
      - score

  disk_fio:
    enabled: true
    tool: fio
    safety:
      # Empêcher un bench destructif ou trop long
      max_runtime_s: 60
      max_size: "1G"
      direct: 1
    params:
      name: "bench"
      ioengine: "libaio"
      rw: "randrw"
      bs: "4k"
      size: "500M"
      numjobs: 1
      runtime_s: 30
      time_based: true
      output_format: "json"
    outputs:
      - read_mb_s
      - write_mb_s
      - iops_read
      - iops_write
      - latency_ms
      - score

  network_iperf3:
    enabled: true
    tool: iperf3
    server: "10.0.0.50"
    port: 5201
    prechecks:
      ping:
        enabled: true
        count: 1
        timeout_s: 1
      port_check:
        enabled: true
        tool: nc
        timeout_s: 2
    params:
      duration_s: 10
      bidir: true
      json: true
    outputs:
      - upload_mbps
      - download_mbps
      - ping_ms
      - score
      # placeholders (comme ton script)
      - jitter_ms
      - packet_loss_percent

  gpu:
    enabled: false
    note: "GPU bench non implémenté dans le script d'origine (placeholder)."

payload_mapping:
  # Le binaire peut mapper ses structures internes vers le schéma backend actuel.
  # Utile si ton backend attend des champs précis.
  device_identifier: "system.hostname"
  bench_script_version_field: "bench_client_version"
  include_sections:
    - hardware
    - results
    - raw_info

limits:
  # Bornes générales de sécurité (validation côté client)
  max_payload_kb: 1024
  max_raw_info_kb: 5120
  max_fio_runtime_s: 60
  max_fio_size_bytes: 1073741824      # 1 GiB
  max_sysbench_cpu_prime: 50000
  max_iperf_duration_s: 30

features:
  # Permet d'activer/désactiver rapidement des blocs selon machines
  enable_screen_resolution_detection: true
  enable_battery_detection: true
  enable_network_share_detection: true
  enable_audio_detection: true
  enable_proxmox_detection: true

[DEBUG] Config chargée : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] Configuration complète : {ConfigVersion:1 Backend:{URL:http://10.0.0.50:8007/api/benchmark Auth:{Mode:bearer_env EnvVar:test_hardware_perf} HTTP:{TimeoutS:15 Retries:2 RetryBackoffS:2 TLSVerify:false}} Runtime:{MaxTotalRuntime:480 CommandTimeout:30 TempDir:/tmp Locale:C PathPrepend:[/usr/sbin /sbin]} Logging:{Level:info Progress:true ShowCommandLines:false CaptureRawOutput:true RawOutputMaxKB:5120 SavePayloadToTmp:true PayloadTmpDir:/tmp PayloadFilenamePrefix:bench_payload_ InteractiveDebugPause:true} Payload:{Dir:. Prefix:bench_payload_ Always:true} Benchmarks:{Enabled:true Weights:map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1] CPU:{Enabled:true Tool:sysbench Server: Port:0 Params:map[cpu_max_prime:20000 multi_threads:all single_thread:1] Safety:map[]} Memory:{Enabled:true Tool:sysbench Server: Port:0 Params:map[total_size:1G] Safety:map[]} Disk:{Enabled:true Tool:fio Server: Port:0 Params:map[bs:4k ioengine:libaio name:bench numjobs:1 output_format:json runtime_s:30 rw:randrw size:500M time_based:true] Safety:map[direct:1 max_runtime_s:60 max_size:1G]} Network:{Enabled:true Tool:iperf3 Server:10.0.0.50 Port:5201 Params:map[bidir:true duration_s:10 json:true] Safety:map[]}} Collection:{System:{Enabled:true} CPU:{Enabled:true} RAM:{Enabled:true} Storage:{Enabled:true} Network:{Enabled:true} GPU:{Enabled:true} Audio:{Enabled:true} PCI:{Enabled:true} USB:{Enabled:true}} RawInfo:{Enabled:true Include:[lscpu lsblk dmidecode] MaxSizeKB:5120}}
[DEBUG] [2/6] Début collecte CPU
[DEBUG] Exec: lscpu []
[DEBUG] Exec: dmidecode [-t 4]
[DEBUG] [2/6] Détails CPU: {Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>}
[DEBUG] [2/6] Début collecte RAM
[DEBUG] SMBIOS détecté : SMBIOS 3.3.0 (54 tables)
[DEBUG] [SMBIOS RAW] Handle=%!s(uint16=11) slots_byte=0x4 (4)
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Module SMBIOS détecté : DIMM 0 {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  }
[DEBUG] Module SMBIOS détecté : DIMM 1 {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}
[DEBUG] Mémoire SMBIOS : slots_total=4 slots_used=4 ecc=false max=131072MB
[DEBUG] RAM result: max=131072MB slotsTotal=4 slotsUsed=4 layout=4 modules
[DEBUG] [2/6] Détails RAM: {TotalMB:48096 UsedMB:18433 FreeMB:29663 SharedMB:996 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]}
[DEBUG] [2/6] Début collecte GPU
[DEBUG] Exec: lspci []
[DEBUG] Exec: nvidia-smi [--query-gpu=name,driver_version,memory.total --format=csv,noheader,nounits]
[DEBUG] [2/6] Détails GPU: {Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc00011a048 MemorySharedMB:<nil> APISupport:[]}
[DEBUG] [2/6] Début collecte stockage
[DEBUG] Exec: lsblk [-J -b -o NAME,TYPE,TRAN,VENDOR,MODEL,SERIAL,SIZE]
[DEBUG] SMART open /dev/sdb impossible: unknown drive type
[DEBUG] SMART open /dev/sdc impossible: unknown drive type
[DEBUG] SMART open /dev/sdd impossible: unknown drive type
[DEBUG] SMART open /dev/sde impossible: unknown drive type
[DEBUG] [2/6] Détails stockage: {Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00011a308 FreeGB:0xc00011a310} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00011a318 FreeGB:0xc00011a350}]}
[DEBUG] [2/6] Début collecte PCI devices
[DEBUG] Exec: lspci [-mm]
[DEBUG] [2/6] Détails PCI: [{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}]
[DEBUG] [2/6] Début collecte USB devices
[DEBUG] Exec: lsusb []
[DEBUG] [2/6] Détails USB: [{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}]
[DEBUG] [2/6] Début collecte partages réseau
[DEBUG] [2/6] Détails partages réseau: []
[DEBUG] [2/6] Début collecte interfaces réseau
[DEBUG] Exec: ethtool [eno1]
[DEBUG] Exec: ethtool [-i eno1]
[DEBUG] Exec: ethtool [wlxe84e06a6c1fc]
[DEBUG] Exec: ethtool [-i wlxe84e06a6c1fc]
[DEBUG] Exec: iwgetid [wlxe84e06a6c1fc -r]
[DEBUG] Exec: iw [wlxe84e06a6c1fc link]
[DEBUG] [2/6] Détails réseau: {Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc00059a3f0 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:ba:c8:d3:a7:be:c8 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]}
[DEBUG] [2/6] Début collecte carte mère
[DEBUG] Exec: dmidecode [-t 2]
[DEBUG] Exec: dmidecode [-t 0]
[DEBUG] [2/6] Détails carte mère: {Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023}
[DEBUG] [2/6] Début collecte OS
[DEBUG] Exec: uname [-r]
[DEBUG] Exec: uname [-m]
[DEBUG] Exec: systemd-detect-virt []
[DEBUG] Exec: xrandr []
[DEBUG] Exec: xrandr [--current]
[DEBUG] Exec: who [-b]
[DEBUG] [2/6] Détails OS: {Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:51459.3 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME}
[DEBUG] [2/6] Début collecte capteurs
[DEBUG] [2/6] Détails capteurs: {CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:53.25 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:37.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:32.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false}]}
[DEBUG] [2/6] Début collecte audio
[DEBUG] Exec: lspci []
[DEBUG] Exec: aplay [-l]
[DEBUG] Exec: arecord [-l]
[DEBUG] Exec: aplay [-L]
[DEBUG] Exec: pactl [info]
[DEBUG] [2/6] Détails audio: {Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}}
[DEBUG] Exec: lscpu []
[DEBUG] Exec: lsblk [-a]
[DEBUG] Exec: dmidecode [-t 0,1,2,16,17]
[DEBUG] Matériel collecté : {CPU:{Vendor:AuthenticAMD Model:AMD Ryzen 9 5900X 12-Core Processor Cores:12 Threads:24 BaseFreqGHz:4.95 MaxFreqGHz:4.95 CacheL1KB:64 CacheL2KB:512 CacheL3KB:32768 Flags:[fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap] Microarchitecture:Zen TDPW:<nil>} RAM:{TotalMB:48096 UsedMB:18433 FreeMB:29663 SharedMB:996 SlotsTotal:4 SlotsUsed:4 MaxCapacityMB:131072 ECC:false Layout:[{Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE} {Slot:DIMM 0 SizeMB:16384 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:2 Manufacturer:Unknown PartNumber:CMW32GX4M2E3200C16  } {Slot:DIMM 1 SizeMB:8192 Type:DDR4 SpeedMHz:3200 ConfiguredMHz:3200 FormFactor:DIMM TypeDetail:Synchronous Unbuffered (Unregistered) Rank:1 Manufacturer:Unknown PartNumber:BL8G32C16U4BL.M8FE}]} GPU:{Vendor:NVIDIA Model:NVIDIA GeForce RTX 3060 DriverVersion:550.163.01 MemoryDedicatedMB:0xc00011a048 MemorySharedMB:<nil> APISupport:[]} Storage:{Devices:[{Name:/dev/nvme0n1 Type:ssd Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2138E5D60DD8 SmartHealth:PASSED Temperature:34} {Name:/dev/nvme1n1 Type: Interface:nvme CapacityGB:465.7617416381836 Vendor:CT500P2SSD8 Model:CT500P2SSD8 Serial:2108E4FD258D SmartHealth:PASSED Temperature:32} {Name:/dev/sda Type: Interface:sata CapacityGB:447.13167572021484 Vendor:ATA      Model:KINGSTON SUV500480G Serial:50026B768226A365 SmartHealth:PASSED Temperature:25} {Name:/dev/sdb Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:Compact Flash Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdc Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:SD/MMC Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sdd Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:MS/MS-PRO Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0} {Name:/dev/sde Type: Interface:usb CapacityGB:0 Vendor:Generic- Model:xD-Picture Serial:058F63626479 SmartHealth:UNAVAILABLE Temperature:0}] Partitions:[{Name:/dev/nvme0n1p2 MountPoint:/ FSType:ext4 TotalGB:432.80120849609375 UsedGB:0xc00011a308 FreeGB:0xc00011a310} {Name:/dev/nvme0n1p1 MountPoint:/boot/efi FSType:vfat TotalGB:0.9512481689453125 UsedGB:0xc00011a318 FreeGB:0xc00011a350}]} PCIDevices:[{Slot:00:00.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Root Complex} {Slot:00:00.2 Class:IOMMU Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse IOMMU} {Slot:00:01.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:01.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:01.3 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:02.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:03.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse GPP Bridge} {Slot:00:04.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:05.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:07.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:08.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Host Bridge} {Slot:00:08.1 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]} {Slot:00:14.0 Class:SMBus Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH SMBus Controller} {Slot:00:14.3 Class:ISA bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:FCH LPC Bridge} {Slot:00:18.0 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 0} {Slot:00:18.1 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 1} {Slot:00:18.2 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 2} {Slot:00:18.3 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 3} {Slot:00:18.4 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 4} {Slot:00:18.5 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 5} {Slot:00:18.6 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 6} {Slot:00:18.7 Class:Host bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse/Vermeer Data Fabric: Device 18h; Function 7} {Slot:01:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:02:00.0 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset USB 3.1 xHCI Compliant Host Controller} {Slot:02:00.1 Class:SATA controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset SATA Controller} {Slot:02:00.2 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Bridge} {Slot:03:00.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:01.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:04.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:03:08.0 Class:PCI bridge Vendor:Advanced Micro Devices, Inc. [AMD] Device:400 Series Chipset PCIe Port} {Slot:04:00.0 Class:Ethernet controller Vendor:Realtek Semiconductor Co., Ltd. Device:RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller} {Slot:07:00.0 Class:Non-Volatile memory controller Vendor:Micron/Crucial Technology Device:P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)} {Slot:08:00.0 Class:VGA compatible controller Vendor:NVIDIA Corporation Device:GA106 [GeForce RTX 3060 Lite Hash Rate]} {Slot:08:00.1 Class:Audio device Vendor:NVIDIA Corporation Device:GA106 High Definition Audio Controller} {Slot:09:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse PCIe Dummy Function} {Slot:0a:00.0 Class:Non-Essential Instrumentation [1300] Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Reserved SPP} {Slot:0a:00.1 Class:Encryption controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse Cryptographic Coprocessor PSPCPP} {Slot:0a:00.3 Class:USB controller Vendor:Advanced Micro Devices, Inc. [AMD] Device:Matisse USB 3.0 Host Controller} {Slot:0a:00.4 Class:Audio device Vendor:Advanced Micro Devices, Inc. [AMD] Device:Starship/Matisse HD Audio Controller}] USBDevices:[{Bus:001 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:001 Device:002 VendorID:058f ProductID:6362 Name:Alcor Micro Corp. Flash Card Reader/Writer} {Bus:002 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub} {Bus:003 Device:001 VendorID:1d6b ProductID:0002 Name:Linux Foundation 2.0 root hub} {Bus:003 Device:003 VendorID:046d ProductID:c52b Name:Logitech, Inc. Unifying Receiver} {Bus:003 Device:004 VendorID:0bda ProductID:b711 Name:Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)} {Bus:004 Device:001 VendorID:1d6b ProductID:0003 Name:Linux Foundation 3.0 root hub}] NetworkShares:[] Network:{Interfaces:[{Name:eno1 Type:ethernet MAC:18:c0:4d:b5:65:74 IP:10.0.1.109 SpeedMbps:0xc00059a3f0 Driver:r8169 SSID: WakeOnLAN:false} {Name:wlxe84e06a6c1fc Type:wifi MAC:ba:c8:d3:a7:be:c8 IP: SpeedMbps:<nil> Driver:rtl8xxxu SSID: WakeOnLAN:false}]} Motherboard:{Vendor:Gigabyte Technology Co., Ltd. Model:B450 AORUS ELITE BIOSVendor:American Megatrends International, LLC. BIOSVersion:F65e BIOSDate:09/20/2023} OS:{Name:Debian GNU/Linux Version:13 (trixie) KernelVersion:6.12.57+deb13-amd64 Architecture:x86_64 SessionType: DisplayServer: ScreenResolution:5560 x 1920 LastBootTime:démarrage système 2026-01-11 09:11 UptimeSeconds:51459.3 BatteryPercentage:<nil> BatteryStatus: BatteryHealth: Hostname:aorus VirtualizationType:kvm-host DesktopEnvironment:GNOME} Sensors:{CPUTempC:<nil> DiskTempsC:map[nvme-pci-0100:Composite:33.85 nvme-pci-0700:Composite:31.85] Sensors:[{Chip:k10temp-pci-00c3 Name:Tctl Type:temperature Value:53.25 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd1 Type:temperature Value:37.5 Unit:°C Alarm:false} {Chip:k10temp-pci-00c3 Name:Tccd2 Type:temperature Value:32.5 Unit:°C Alarm:false} {Chip:nvme-pci-0100 Name:Composite Type:temperature Value:33.85 Unit:°C Alarm:false} {Chip:nvme-pci-0700 Name:Composite Type:temperature Value:31.85 Unit:°C Alarm:false} {Chip:acpitz-acpi-0 Name:temp1 Type:temperature Value:16.8 Unit:°C Alarm:false}]} Audio:{Hardware:{PCIAudioDevices:[08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1) 0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller] AlsaPlayback:**** Liste des périphériques matériels PLAYBACK ****
carte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 AlsaCapture:**** Liste des périphériques matériels CAPTURE ****
carte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
carte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]
  Sous-périphériques : 1/1
  Sous-périphérique #0 : subdevice #0
 PCMDevices:[null Discard all samples (playback) or generate zero samples (capture) pipewire PipeWire Sound Server default Default ALSA Output (currently PipeWire Media Server) hw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct hardware device without any conversions hw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct hardware device without any conversions hw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct hardware device without any conversions hw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct hardware device without any conversions plughw:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Hardware device with all software conversions plughw:CARD=NVidia,DEV=7 HDA NVidia, K243Y Hardware device with all software conversions plughw:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Hardware device with all software conversions plughw:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Hardware device with all software conversions hdmi:CARD=NVidia,DEV=0 HDA NVidia, LG ULTRAWIDE HDMI Audio Output hdmi:CARD=NVidia,DEV=1 HDA NVidia, K243Y HDMI Audio Output hdmi:CARD=NVidia,DEV=2 HDA NVidia, HDMI 2 HDMI Audio Output hdmi:CARD=NVidia,DEV=3 HDA NVidia, HDMI 3 HDMI Audio Output dmix:CARD=NVidia,DEV=3 HDA NVidia, LG ULTRAWIDE Direct sample mixing device dmix:CARD=NVidia,DEV=7 HDA NVidia, K243Y Direct sample mixing device dmix:CARD=NVidia,DEV=8 HDA NVidia, HDMI 2 Direct sample mixing device dmix:CARD=NVidia,DEV=9 HDA NVidia, HDMI 3 Direct sample mixing device hw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct hardware device without any conversions hw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct hardware device without any conversions plughw:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Hardware device with all software conversions plughw:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Hardware device with all software conversions sysdefault:CARD=Generic HD-Audio Generic, ALC892 Analog Default Audio Device front:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Front output / input surround21:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 2.1 Surround output to Front and Subwoofer speakers surround40:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.0 Surround output to Front and Rear speakers surround41:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 4.1 Surround output to Front, Rear and Subwoofer speakers surround50:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.0 Surround output to Front, Center and Rear speakers surround51:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 5.1 Surround output to Front, Center, Rear and Subwoofer speakers surround71:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog 7.1 Surround output to Front, Center, Side, Rear and Woofer speakers iec958:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Digital IEC958 (S/PDIF) Digital Audio Output dmix:CARD=Generic,DEV=0 HD-Audio Generic, ALC892 Analog Direct sample mixing device dmix:CARD=Generic,DEV=1 HD-Audio Generic, ALC892 Digital Direct sample mixing device]} Software:{Backend: ServerName: ServerVersion: DefaultSink:<nil> DefaultSource:<nil> Sinks:[] Sources:[]}} RawInfo:map[dmidecode:# dmidecode 3.6
Getting SMBIOS data from sysfs.
SMBIOS 3.3.0 present.

Handle 0x0000, DMI type 0, 26 bytes
BIOS Information
	Vendor: American Megatrends International, LLC.
	Version: F65e
	Release Date: 09/20/2023
	Address: 0xF0000
	Runtime Size: 64 kB
	ROM Size: 16 MB
	Characteristics:
		PCI is supported
		BIOS is upgradeable
		BIOS shadowing is allowed
		Boot from CD is supported
		Selectable boot is supported
		BIOS ROM is socketed
		EDD is supported
		Japanese floppy for NEC 9800 1.2 MB is supported (int 13h)
		Japanese floppy for Toshiba 1.2 MB is supported (int 13h)
		5.25"/360 kB floppy services are supported (int 13h)
		5.25"/1.2 MB floppy services are supported (int 13h)
		3.5"/720 kB floppy services are supported (int 13h)
		3.5"/2.88 MB floppy services are supported (int 13h)
		Print screen service is supported (int 5h)
		Serial services are supported (int 14h)
		Printer services are supported (int 17h)
		CGA/mono video services are supported (int 10h)
		USB legacy is supported
		BIOS boot specification is supported
		Targeted content distribution is supported
		UEFI is supported
	BIOS Revision: 5.17

Handle 0x0001, DMI type 1, 27 bytes
System Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	UUID: 03c00218-044d-05b5-6506-740700080009
	Wake-up Type: Power Switch
	SKU Number: Default string
	Family: B450 MB

Handle 0x0002, DMI type 2, 15 bytes
Base Board Information
	Manufacturer: Gigabyte Technology Co., Ltd.
	Product Name: B450 AORUS ELITE
	Version: Default string
	Serial Number: Default string
	Asset Tag: Default string
	Features:
		Board is a hosting board
		Board is replaceable
	Location In Chassis: Default string
	Chassis Handle: 0x0003
	Type: Motherboard
	Contained Object Handles: 0

Handle 0x000B, DMI type 16, 23 bytes
Physical Memory Array
	Location: System Board Or Motherboard
	Use: System Memory
	Error Correction Type: None
	Maximum Capacity: 128 GB
	Error Information Handle: 0x000A
	Number Of Devices: 4

Handle 0x0013, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0012
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x0016, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0015
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL A
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C4408B
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

Handle 0x0019, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x0018
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 16 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 0
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: 00000000
	Asset Tag: Not Specified
	Part Number: CMW32GX4M2E3200C16  
	Rank: 2
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: Unknown
	Maximum Voltage: Unknown
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 3, Hex 0x9E
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 16 GB
	Cache Size: None
	Logical Size: None

Handle 0x001C, DMI type 17, 92 bytes
Memory Device
	Array Handle: 0x000B
	Error Information Handle: 0x001B
	Total Width: 64 bits
	Data Width: 64 bits
	Size: 8 GB
	Form Factor: DIMM
	Set: None
	Locator: DIMM 1
	Bank Locator: P0 CHANNEL B
	Type: DDR4
	Type Detail: Synchronous Unbuffered (Unregistered)
	Speed: 3200 MT/s
	Manufacturer: Unknown
	Serial Number: E3C44087
	Asset Tag: Not Specified
	Part Number: BL8G32C16U4BL.M8FE
	Rank: 1
	Configured Memory Speed: 3200 MT/s
	Minimum Voltage: 1.2 V
	Maximum Voltage: 1.2 V
	Configured Voltage: 1.2 V
	Memory Technology: DRAM
	Memory Operating Mode Capability: Volatile memory
	Firmware Version: Unknown
	Module Manufacturer ID: Bank 6, Hex 0x9B
	Module Product ID: Unknown
	Memory Subsystem Controller Manufacturer ID: Unknown
	Memory Subsystem Controller Product ID: Unknown
	Non-Volatile Size: None
	Volatile Size: 8 GB
	Cache Size: None
	Logical Size: None

 lsblk:NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS
loop0         7:0    0 118,5M  1 loop /snap/iptvnator/92
loop1         7:1    0  48,1M  1 loop /snap/snapd/25935
loop2         7:2    0  50,9M  1 loop /snap/snapd/25577
loop3         7:3    0     4K  1 loop /snap/bare/5
loop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535
loop5         7:5    0  55,5M  1 loop /snap/core18/2976
loop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198
loop7         7:7    0     0B  0 loop 
sda           8:0    0 447,1G  0 disk 
└─sda1        8:1    0 447,1G  0 part 
sdb           8:16   1     0B  0 disk 
sdc           8:32   1     0B  0 disk 
sdd           8:48   1     0B  0 disk 
sde           8:64   1     0B  0 disk 
nvme0n1     259:0    0 465,8G  0 disk 
├─nvme0n1p1 259:1    0   976M  0 part /boot/efi
├─nvme0n1p2 259:2    0 440,8G  0 part /
└─nvme0n1p3 259:3    0    24G  0 part [SWAP]
nvme1n1     259:4    0 465,8G  0 disk 
├─nvme1n1p1 259:5    0    50M  0 part 
├─nvme1n1p2 259:6    0 464,3G  0 part 
├─nvme1n1p3 259:7    0   808M  0 part 
├─nvme1n1p4 259:8    0   100M  0 part 
└─nvme1n1p5 259:9    0   522M  0 part 
 lscpu:Architecture :                            x86_64
Mode(s) opératoire(s) des processeurs :   32-bit, 64-bit
Tailles des adresses:                     48 bits physical, 48 bits virtual
Boutisme :                                Little Endian
Processeur(s) :                           24
Liste de processeur(s) en ligne :         0-23
Identifiant constructeur :                AuthenticAMD
Nom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor
Famille de processeur :                   25
Modèle :                                  33
Thread(s) par cœur :                      2
Cœur(s) par socket :                      12
Socket(s) :                               1
Révision :                                2
Accroissement de fréquence :              activé
multiplication des MHz du/des CPU(s) :    96%
Vitesse maximale du processeur en MHz :   4951,0000
Vitesse minimale du processeur en MHz :   550,0000
BogoMIPS :                                7399,98
Drapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap
Virtualisation :                          AMD-V
Cache L1d :                               384 KiB (12 instances)
Cache L1i :                               384 KiB (12 instances)
Cache L2 :                                6 MiB (12 instances)
Cache L3 :                                64 MiB (2 instances)
Nœud(s) NUMA :                            1
Nœud NUMA 0 de processeur(s) :            0-23
Vulnérabilité Gather data sampling :      Not affected
Vulnérabilité Indirect target selection : Not affected
Vulnérabilité Itlb multihit :             Not affected
Vulnérabilité L1tf :                      Not affected
Vulnérabilité Mds :                       Not affected
Vulnérabilité Meltdown :                  Not affected
Vulnérabilité Mmio stale data :           Not affected
Vulnérabilité Reg file data sampling :    Not affected
Vulnérabilité Retbleed :                  Not affected
Vulnérabilité Spec rstack overflow :      Mitigation; Safe RET
Vulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl
Vulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization
Vulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected
Vulnérabilité Srbds :                     Not affected
Vulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode
Vulnérabilité Tsx async abort :           Not affected
Vulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace
]}
[DEBUG] [3/6] Benchmark CPU démarré
[DEBUG] Exec: sysbench [cpu --threads=1 --time=10 run]
[DEBUG] Exec: nproc []
[DEBUG] Exec: sysbench [cpu --threads=24 --time=10 run]
[DEBUG] [3/6] Résultat CPU: {EventsPerSec:37357.46 EventsPerSecSingle:5582.37 EventsPerSecMulti:69132.56 DurationSec:20 Score:37357.46 ScoreSingle:5582.37 ScoreMulti:69132.56}
[DEBUG] [3/6] Benchmark mémoire démarré
[DEBUG] Exec: sysbench [memory --memory-block-size=1K --memory-total-size=1G run]
[DEBUG] [3/6] Résultat mémoire: {Throughput:8702.43 Score:8702.43}
[DEBUG] [3/6] Benchmark disque démarré
[DEBUG] [3/6] Bench disque cible : /var/tmp/bench-client (mount=/ fstype=ext4 source=/dev/nvme0n1p2)
[DEBUG] [3/6] Bench disque direct sur /dev/nvme0n1p2 (mnt=/ fs=ext4)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-500mb.bin (500 MB)
[DEBUG] [3/6] Bench direct : écriture+lecture /var/tmp/bench-client/direct-1gb.bin (1024 MB)
[DEBUG] [3/6] Bench direct chunk 1/50 (/var/tmp/bench-client/direct-chunk-01.bin)
[DEBUG] [3/6] Bench direct chunk 2/50 (/var/tmp/bench-client/direct-chunk-02.bin)
[DEBUG] [3/6] Bench direct chunk 3/50 (/var/tmp/bench-client/direct-chunk-03.bin)
[DEBUG] [3/6] Bench direct chunk 4/50 (/var/tmp/bench-client/direct-chunk-04.bin)
[DEBUG] [3/6] Bench direct chunk 5/50 (/var/tmp/bench-client/direct-chunk-05.bin)
[DEBUG] [3/6] Bench direct chunk 6/50 (/var/tmp/bench-client/direct-chunk-06.bin)
[DEBUG] [3/6] Bench direct chunk 7/50 (/var/tmp/bench-client/direct-chunk-07.bin)
[DEBUG] [3/6] Bench direct chunk 8/50 (/var/tmp/bench-client/direct-chunk-08.bin)
[DEBUG] [3/6] Bench direct chunk 9/50 (/var/tmp/bench-client/direct-chunk-09.bin)
[DEBUG] [3/6] Bench direct chunk 10/50 (/var/tmp/bench-client/direct-chunk-10.bin)
[DEBUG] [3/6] Bench direct chunk 11/50 (/var/tmp/bench-client/direct-chunk-11.bin)
[DEBUG] [3/6] Bench direct chunk 12/50 (/var/tmp/bench-client/direct-chunk-12.bin)
[DEBUG] [3/6] Bench direct chunk 13/50 (/var/tmp/bench-client/direct-chunk-13.bin)
[DEBUG] [3/6] Bench direct chunk 14/50 (/var/tmp/bench-client/direct-chunk-14.bin)
[DEBUG] [3/6] Bench direct chunk 15/50 (/var/tmp/bench-client/direct-chunk-15.bin)
[DEBUG] [3/6] Bench direct chunk 16/50 (/var/tmp/bench-client/direct-chunk-16.bin)
[DEBUG] [3/6] Bench direct chunk 17/50 (/var/tmp/bench-client/direct-chunk-17.bin)
[DEBUG] [3/6] Bench direct chunk 18/50 (/var/tmp/bench-client/direct-chunk-18.bin)
[DEBUG] [3/6] Bench direct chunk 19/50 (/var/tmp/bench-client/direct-chunk-19.bin)
[DEBUG] [3/6] Bench direct chunk 20/50 (/var/tmp/bench-client/direct-chunk-20.bin)
[DEBUG] [3/6] Bench direct chunk 21/50 (/var/tmp/bench-client/direct-chunk-21.bin)
[DEBUG] [3/6] Bench direct chunk 22/50 (/var/tmp/bench-client/direct-chunk-22.bin)
[DEBUG] [3/6] Bench direct chunk 23/50 (/var/tmp/bench-client/direct-chunk-23.bin)
[DEBUG] [3/6] Bench direct chunk 24/50 (/var/tmp/bench-client/direct-chunk-24.bin)
[DEBUG] [3/6] Bench direct chunk 25/50 (/var/tmp/bench-client/direct-chunk-25.bin)
[DEBUG] [3/6] Bench direct chunk 26/50 (/var/tmp/bench-client/direct-chunk-26.bin)
[DEBUG] [3/6] Bench direct chunk 27/50 (/var/tmp/bench-client/direct-chunk-27.bin)
[DEBUG] [3/6] Bench direct chunk 28/50 (/var/tmp/bench-client/direct-chunk-28.bin)
[DEBUG] [3/6] Bench direct chunk 29/50 (/var/tmp/bench-client/direct-chunk-29.bin)
[DEBUG] [3/6] Bench direct chunk 30/50 (/var/tmp/bench-client/direct-chunk-30.bin)
[DEBUG] [3/6] Bench direct chunk 31/50 (/var/tmp/bench-client/direct-chunk-31.bin)
[DEBUG] [3/6] Bench direct chunk 32/50 (/var/tmp/bench-client/direct-chunk-32.bin)
[DEBUG] [3/6] Bench direct chunk 33/50 (/var/tmp/bench-client/direct-chunk-33.bin)
[DEBUG] [3/6] Bench direct chunk 34/50 (/var/tmp/bench-client/direct-chunk-34.bin)
[DEBUG] [3/6] Bench direct chunk 35/50 (/var/tmp/bench-client/direct-chunk-35.bin)
[DEBUG] [3/6] Bench direct chunk 36/50 (/var/tmp/bench-client/direct-chunk-36.bin)
[DEBUG] [3/6] Bench direct chunk 37/50 (/var/tmp/bench-client/direct-chunk-37.bin)
[DEBUG] [3/6] Bench direct chunk 38/50 (/var/tmp/bench-client/direct-chunk-38.bin)
[DEBUG] [3/6] Bench direct chunk 39/50 (/var/tmp/bench-client/direct-chunk-39.bin)
[DEBUG] [3/6] Bench direct chunk 40/50 (/var/tmp/bench-client/direct-chunk-40.bin)
[DEBUG] [3/6] Bench direct chunk 41/50 (/var/tmp/bench-client/direct-chunk-41.bin)
[DEBUG] [3/6] Bench direct chunk 42/50 (/var/tmp/bench-client/direct-chunk-42.bin)
[DEBUG] [3/6] Bench direct chunk 43/50 (/var/tmp/bench-client/direct-chunk-43.bin)
[DEBUG] [3/6] Bench direct chunk 44/50 (/var/tmp/bench-client/direct-chunk-44.bin)
[DEBUG] [3/6] Bench direct chunk 45/50 (/var/tmp/bench-client/direct-chunk-45.bin)
[DEBUG] [3/6] Bench direct chunk 46/50 (/var/tmp/bench-client/direct-chunk-46.bin)
[DEBUG] [3/6] Bench direct chunk 47/50 (/var/tmp/bench-client/direct-chunk-47.bin)
[DEBUG] [3/6] Bench direct chunk 48/50 (/var/tmp/bench-client/direct-chunk-48.bin)
[DEBUG] [3/6] Bench direct chunk 49/50 (/var/tmp/bench-client/direct-chunk-49.bin)
[DEBUG] [3/6] Bench direct chunk 50/50 (/var/tmp/bench-client/direct-chunk-50.bin)
[DEBUG] [3/6] Bench disque direct résumé -> write=969.78 MB/s read=15024.73 MB/s
[DEBUG] Exec: fio [--name=bench --ioengine=libaio --rw=randrw --bs=4k --direct=1 --size=500M --numjobs=1 --runtime=30 --time_based --output-format=json --filename=/var/tmp/bench-client/bench-1768170593596690760.fio]
[DEBUG] [3/6] Bench disque final -> read=15024.73 MB/s write=969.78 MB/s score=7997.26
[DEBUG] [3/6] Résultat disque: {ReadMBs:15024.73 WriteMBs:969.78 IOPSRead:10212.69 IOPSWrite:10206.29 LatencyMs:0.07 Score:7997.26}
[DEBUG] [3/6] Benchmark réseau démarré
[DEBUG] Exec: iperf3 [-c 10.0.0.50 -p 5201 -J -t 10]
[DEBUG] Exec: ping [-c 1 -W 1 10.0.0.50]
[DEBUG] [3/6] Résultat réseau: {Upload:942.03 Download:939.17 PingMs:0.35 JitterMs:<nil> PacketLossPct:<nil> Score:940.6}
[DEBUG] Résultats des benchmarks : {CPU:{EventsPerSec:37357.46 EventsPerSecSingle:5582.37 EventsPerSecMulti:69132.56 DurationSec:20 Score:37357.46 ScoreSingle:5582.37 ScoreMulti:69132.56} Memory:{Throughput:8702.43 Score:8702.43} Disk:{ReadMBs:15024.73 WriteMBs:969.78 IOPSRead:10212.69 IOPSWrite:10206.29 LatencyMs:0.07 Score:7997.26} Network:{Upload:942.03 Download:939.17 PingMs:0.35 JitterMs:<nil> PacketLossPct:<nil> Score:940.6} GPU:{GLMark2Score:<nil> Score:<nil>} GlobalScore:0}
[DEBUG] Poids benchmarks : map[cpu:0.4 disk:0.2 gpu:0.1 memory:0.2 network:0.1]
[DEBUG] Scores normalisés : cpu=1867.87 mem=87.02 disk=799.73 net=94.06
[DEBUG] Score global calculé : 93390.54
[DEBUG] Payload JSON (49098 octets) : {
  "device_identifier": "aorus",
  "bench_script_version": "1.6.6",
  "bench_client_version": "1.0.2",
  "hardware": {
    "cpu": {
      "vendor": "AuthenticAMD",
      "model": "AMD Ryzen 9 5900X 12-Core Processor",
      "cores": 12,
      "threads": 24,
      "base_freq_ghz": 4.95,
      "max_freq_ghz": 4.95,
      "cache_l1_kb": 64,
      "cache_l2_kb": 512,
      "cache_l3_kb": 32768,
      "flags": [
        "fpu",
        "vme",
        "de",
        "pse",
        "tsc",
        "msr",
        "pae",
        "mce",
        "cx8",
        "apic",
        "sep",
        "mtrr",
        "pge",
        "mca",
        "cmov",
        "pat",
        "pse36",
        "clflush",
        "mmx",
        "fxsr",
        "sse",
        "sse2",
        "ht",
        "syscall",
        "nx",
        "mmxext",
        "fxsr_opt",
        "pdpe1gb",
        "rdtscp",
        "lm",
        "constant_tsc",
        "rep_good",
        "nopl",
        "xtopology",
        "nonstop_tsc",
        "cpuid",
        "extd_apicid",
        "aperfmperf",
        "rapl",
        "pni",
        "pclmulqdq",
        "monitor",
        "ssse3",
        "fma",
        "cx16",
        "sse4_1",
        "sse4_2",
        "x2apic",
        "movbe",
        "popcnt",
        "aes",
        "xsave",
        "avx",
        "f16c",
        "rdrand",
        "lahf_lm",
        "cmp_legacy",
        "svm",
        "extapic",
        "cr8_legacy",
        "abm",
        "sse4a",
        "misalignsse",
        "3dnowprefetch",
        "osvw",
        "ibs",
        "skinit",
        "wdt",
        "tce",
        "topoext",
        "perfctr_core",
        "perfctr_nb",
        "bpext",
        "perfctr_llc",
        "mwaitx",
        "cpb",
        "cat_l3",
        "cdp_l3",
        "hw_pstate",
        "ssbd",
        "mba",
        "ibrs",
        "ibpb",
        "stibp",
        "vmmcall",
        "fsgsbase",
        "bmi1",
        "avx2",
        "smep",
        "bmi2",
        "erms",
        "invpcid",
        "cqm",
        "rdt_a",
        "rdseed",
        "adx",
        "smap",
        "clflushopt",
        "clwb",
        "sha_ni",
        "xsaveopt",
        "xsavec",
        "xgetbv1",
        "xsaves",
        "cqm_llc",
        "cqm_occup_llc",
        "cqm_mbm_total",
        "cqm_mbm_local",
        "user_shstk",
        "clzero",
        "irperf",
        "xsaveerptr",
        "rdpru",
        "wbnoinvd",
        "arat",
        "npt",
        "lbrv",
        "svm_lock",
        "nrip_save",
        "tsc_scale",
        "vmcb_clean",
        "flushbyasid",
        "decodeassists",
        "pausefilter",
        "pfthreshold",
        "avic",
        "v_vmsave_vmload",
        "vgif",
        "v_spec_ctrl",
        "umip",
        "pku",
        "ospke",
        "vaes",
        "vpclmulqdq",
        "rdpid",
        "overflow_recov",
        "succor",
        "smca",
        "fsrm",
        "debug_swap"
      ],
      "microarchitecture": "Zen",
      "tdp_w": null
    },
    "ram": {
      "total_mb": 48096,
      "used_mb": 18433,
      "free_mb": 29663,
      "shared_mb": 996,
      "slots_total": 4,
      "slots_used": 4,
      "max_capacity_mb": 131072,
      "ecc": false,
      "layout": [
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        },
        {
          "slot": "DIMM 0",
          "size_mb": 16384,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "2",
          "manufacturer": "Unknown",
          "part_number": "CMW32GX4M2E3200C16  "
        },
        {
          "slot": "DIMM 1",
          "size_mb": 8192,
          "type": "DDR4",
          "speed_mhz": 3200,
          "configured_speed_mhz": 3200,
          "form_factor": "DIMM",
          "type_detail": "Synchronous Unbuffered (Unregistered)",
          "rank": "1",
          "manufacturer": "Unknown",
          "part_number": "BL8G32C16U4BL.M8FE"
        }
      ]
    },
    "gpu": {
      "vendor": "NVIDIA",
      "model": "NVIDIA GeForce RTX 3060",
      "driver_version": "550.163.01",
      "memory_dedicated_mb": 12288,
      "memory_shared_mb": null,
      "api_support": null
    },
    "storage": {
      "devices": [
        {
          "name": "/dev/nvme0n1",
          "type": "ssd",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2138E5D60DD8",
          "smart_health": "PASSED",
          "temperature_c": 34
        },
        {
          "name": "/dev/nvme1n1",
          "type": "",
          "interface": "nvme",
          "capacity_gb": 465.7617416381836,
          "vendor": "CT500P2SSD8",
          "model": "CT500P2SSD8",
          "serial": "2108E4FD258D",
          "smart_health": "PASSED",
          "temperature_c": 32
        },
        {
          "name": "/dev/sda",
          "type": "",
          "interface": "sata",
          "capacity_gb": 447.13167572021484,
          "vendor": "ATA     ",
          "model": "KINGSTON SUV500480G",
          "serial": "50026B768226A365",
          "smart_health": "PASSED",
          "temperature_c": 25
        },
        {
          "name": "/dev/sdb",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "Compact Flash",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdc",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "SD/MMC",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sdd",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "MS/MS-PRO",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        },
        {
          "name": "/dev/sde",
          "type": "",
          "interface": "usb",
          "capacity_gb": 0,
          "vendor": "Generic-",
          "model": "xD-Picture",
          "serial": "058F63626479",
          "smart_health": "UNAVAILABLE",
          "temperature_c": 0
        }
      ],
      "partitions": [
        {
          "name": "/dev/nvme0n1p2",
          "mount_point": "/",
          "fs_type": "ext4",
          "total_gb": 432.80120849609375,
          "used_gb": 349.38393783569336,
          "free_gb": 61.36209487915039
        },
        {
          "name": "/dev/nvme0n1p1",
          "mount_point": "/boot/efi",
          "fs_type": "vfat",
          "total_gb": 0.9512481689453125,
          "used_gb": 0.008571624755859375,
          "free_gb": 0.9426765441894531
        }
      ]
    },
    "pci_devices": [
      {
        "slot": "00:00.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Root Complex"
      },
      {
        "slot": "00:00.2",
        "class": "IOMMU",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse IOMMU"
      },
      {
        "slot": "00:01.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:01.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:01.3",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:02.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:03.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse GPP Bridge"
      },
      {
        "slot": "00:04.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:05.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:07.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:08.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Host Bridge"
      },
      {
        "slot": "00:08.1",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Internal PCIe GPP Bridge 0 to bus[E:B]"
      },
      {
        "slot": "00:14.0",
        "class": "SMBus",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH SMBus Controller"
      },
      {
        "slot": "00:14.3",
        "class": "ISA bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "FCH LPC Bridge"
      },
      {
        "slot": "00:18.0",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 0"
      },
      {
        "slot": "00:18.1",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 1"
      },
      {
        "slot": "00:18.2",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 2"
      },
      {
        "slot": "00:18.3",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 3"
      },
      {
        "slot": "00:18.4",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 4"
      },
      {
        "slot": "00:18.5",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 5"
      },
      {
        "slot": "00:18.6",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 6"
      },
      {
        "slot": "00:18.7",
        "class": "Host bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse/Vermeer Data Fabric: Device 18h; Function 7"
      },
      {
        "slot": "01:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "02:00.0",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset USB 3.1 xHCI Compliant Host Controller"
      },
      {
        "slot": "02:00.1",
        "class": "SATA controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset SATA Controller"
      },
      {
        "slot": "02:00.2",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Bridge"
      },
      {
        "slot": "03:00.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:01.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:04.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "03:08.0",
        "class": "PCI bridge",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "400 Series Chipset PCIe Port"
      },
      {
        "slot": "04:00.0",
        "class": "Ethernet controller",
        "vendor": "Realtek Semiconductor Co., Ltd.",
        "device": "RTL8111/8168/8211/8411 PCI Express Gigabit Ethernet Controller"
      },
      {
        "slot": "07:00.0",
        "class": "Non-Volatile memory controller",
        "vendor": "Micron/Crucial Technology",
        "device": "P2 [Nick P2] / P3 / P3 Plus NVMe PCIe SSD (DRAM-less)"
      },
      {
        "slot": "08:00.0",
        "class": "VGA compatible controller",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 [GeForce RTX 3060 Lite Hash Rate]"
      },
      {
        "slot": "08:00.1",
        "class": "Audio device",
        "vendor": "NVIDIA Corporation",
        "device": "GA106 High Definition Audio Controller"
      },
      {
        "slot": "09:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse PCIe Dummy Function"
      },
      {
        "slot": "0a:00.0",
        "class": "Non-Essential Instrumentation [1300]",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Reserved SPP"
      },
      {
        "slot": "0a:00.1",
        "class": "Encryption controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse Cryptographic Coprocessor PSPCPP"
      },
      {
        "slot": "0a:00.3",
        "class": "USB controller",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Matisse USB 3.0 Host Controller"
      },
      {
        "slot": "0a:00.4",
        "class": "Audio device",
        "vendor": "Advanced Micro Devices, Inc. [AMD]",
        "device": "Starship/Matisse HD Audio Controller"
      }
    ],
    "usb_devices": [
      {
        "bus": "001",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "001",
        "device": "002",
        "vendor_id": "058f",
        "product_id": "6362",
        "name": "Alcor Micro Corp. Flash Card Reader/Writer"
      },
      {
        "bus": "002",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      },
      {
        "bus": "003",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0002",
        "name": "Linux Foundation 2.0 root hub"
      },
      {
        "bus": "003",
        "device": "003",
        "vendor_id": "046d",
        "product_id": "c52b",
        "name": "Logitech, Inc. Unifying Receiver"
      },
      {
        "bus": "003",
        "device": "004",
        "vendor_id": "0bda",
        "product_id": "b711",
        "name": "Realtek Semiconductor Corp. RTL8188GU 802.11n WLAN Adapter (After Modeswitch)"
      },
      {
        "bus": "004",
        "device": "001",
        "vendor_id": "1d6b",
        "product_id": "0003",
        "name": "Linux Foundation 3.0 root hub"
      }
    ],
    "network_shares": [],
    "network": {
      "interfaces": [
        {
          "name": "eno1",
          "type": "ethernet",
          "mac": "18:c0:4d:b5:65:74",
          "ip": "10.0.1.109",
          "speed_mbps": 1000,
          "driver": "r8169",
          "ssid": "",
          "wake_on_lan": false
        },
        {
          "name": "wlxe84e06a6c1fc",
          "type": "wifi",
          "mac": "ba:c8:d3:a7:be:c8",
          "ip": "",
          "speed_mbps": null,
          "driver": "rtl8xxxu",
          "ssid": "",
          "wake_on_lan": false
        }
      ]
    },
    "motherboard": {
      "vendor": "Gigabyte Technology Co., Ltd.",
      "model": "B450 AORUS ELITE",
      "bios_vendor": "American Megatrends International, LLC.",
      "bios_version": "F65e",
      "bios_date": "09/20/2023"
    },
    "os": {
      "name": "Debian GNU/Linux",
      "version": "13 (trixie)",
      "kernel_version": "6.12.57+deb13-amd64",
      "architecture": "x86_64",
      "session_type": "",
      "display_server": "",
      "screen_resolution": "5560 x 1920",
      "last_boot_time": "démarrage système 2026-01-11 09:11",
      "uptime_seconds": 51459.3,
      "battery_percentage": null,
      "battery_status": "",
      "battery_health": "",
      "hostname": "aorus",
      "virtualization_type": "kvm-host",
      "desktop_environment": "GNOME"
    },
    "sensors": {
      "cpu_temp_c": null,
      "disk_temps_c": {
        "nvme-pci-0100:Composite": 33.85,
        "nvme-pci-0700:Composite": 31.85
      },
      "sensors": [
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tctl",
          "type": "temperature",
          "value": 53.25,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd1",
          "type": "temperature",
          "value": 37.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "k10temp-pci-00c3",
          "name": "Tccd2",
          "type": "temperature",
          "value": 32.5,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0100",
          "name": "Composite",
          "type": "temperature",
          "value": 33.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "nvme-pci-0700",
          "name": "Composite",
          "type": "temperature",
          "value": 31.85,
          "unit": "°C",
          "alarm": false
        },
        {
          "chip": "acpitz-acpi-0",
          "name": "temp1",
          "type": "temperature",
          "value": 16.8,
          "unit": "°C",
          "alarm": false
        }
      ]
    },
    "audio": {
      "hardware": {
        "pci_audio_devices": [
          "08:00.1 Audio device: NVIDIA Corporation GA106 High Definition Audio Controller (rev a1)",
          "0a:00.4 Audio device: Advanced Micro Devices, Inc. [AMD] Starship/Matisse HD Audio Controller"
        ],
        "alsa_playback": "**** Liste des périphériques matériels PLAYBACK ****\ncarte 0 : NVidia [HDA NVidia], périphérique 3 : HDMI 0 [LG ULTRAWIDE]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 7 : HDMI 1 [K243Y]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 8 : HDMI 2 [HDMI 2]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 0 : NVidia [HDA NVidia], périphérique 9 : HDMI 3 [HDMI 3]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 1 : ALC892 Digital [ALC892 Digital]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "alsa_capture": "**** Liste des périphériques matériels CAPTURE ****\ncarte 1 : Generic [HD-Audio Generic], périphérique 0 : ALC892 Analog [ALC892 Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\ncarte 1 : Generic [HD-Audio Generic], périphérique 2 : ALC892 Alt Analog [ALC892 Alt Analog]\n  Sous-périphériques : 1/1\n  Sous-périphérique #0 : subdevice #0\n",
        "pcm_devices": [
          "null",
          "Discard all samples (playback) or generate zero samples (capture)",
          "pipewire",
          "PipeWire Sound Server",
          "default",
          "Default ALSA Output (currently PipeWire Media Server)",
          "hw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct hardware device without any conversions",
          "hw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct hardware device without any conversions",
          "plughw:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Hardware device with all software conversions",
          "plughw:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Hardware device with all software conversions",
          "hdmi:CARD=NVidia,DEV=0",
          "HDA NVidia, LG ULTRAWIDE",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=1",
          "HDA NVidia, K243Y",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=2",
          "HDA NVidia, HDMI 2",
          "HDMI Audio Output",
          "hdmi:CARD=NVidia,DEV=3",
          "HDA NVidia, HDMI 3",
          "HDMI Audio Output",
          "dmix:CARD=NVidia,DEV=3",
          "HDA NVidia, LG ULTRAWIDE",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=7",
          "HDA NVidia, K243Y",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=8",
          "HDA NVidia, HDMI 2",
          "Direct sample mixing device",
          "dmix:CARD=NVidia,DEV=9",
          "HDA NVidia, HDMI 3",
          "Direct sample mixing device",
          "hw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct hardware device without any conversions",
          "hw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct hardware device without any conversions",
          "plughw:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Hardware device with all software conversions",
          "plughw:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Hardware device with all software conversions",
          "sysdefault:CARD=Generic",
          "HD-Audio Generic, ALC892 Analog",
          "Default Audio Device",
          "front:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Front output / input",
          "surround21:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "2.1 Surround output to Front and Subwoofer speakers",
          "surround40:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.0 Surround output to Front and Rear speakers",
          "surround41:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "4.1 Surround output to Front, Rear and Subwoofer speakers",
          "surround50:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.0 Surround output to Front, Center and Rear speakers",
          "surround51:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "5.1 Surround output to Front, Center, Rear and Subwoofer speakers",
          "surround71:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "7.1 Surround output to Front, Center, Side, Rear and Woofer speakers",
          "iec958:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Digital",
          "IEC958 (S/PDIF) Digital Audio Output",
          "dmix:CARD=Generic,DEV=0",
          "HD-Audio Generic, ALC892 Analog",
          "Direct sample mixing device",
          "dmix:CARD=Generic,DEV=1",
          "HD-Audio Generic, ALC892 Digital",
          "Direct sample mixing device"
        ]
      },
      "software": {
        "backend": "",
        "server_name": "",
        "server_version": "",
        "default_sink": null,
        "default_source": null,
        "sinks": null,
        "sources": null
      }
    },
    "raw_info": {
      "debug": "active",
      "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
      "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
      "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    96%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
    }
  },
  "results": {
    "cpu": {
      "events_per_sec": 37357.46,
      "events_per_sec_single": 5582.37,
      "events_per_sec_multi": 69132.56,
      "duration_s": 20,
      "score": 37357.46,
      "score_single": 5582.37,
      "score_multi": 69132.56
    },
    "memory": {
      "throughput_mib_s": 8702.43,
      "score": 8702.43
    },
    "disk": {
      "read_mb_s": 15024.73,
      "write_mb_s": 969.78,
      "iops_read": 10212.69,
      "iops_write": 10206.29,
      "latency_ms": 0.07,
      "score": 7997.26
    },
    "network": {
      "upload_mbps": 942.03,
      "download_mbps": 939.17,
      "ping_ms": 0.35,
      "jitter_ms": null,
      "packet_loss_percent": null,
      "score": 940.6
    },
    "gpu": {
      "glmark2_score": null,
      "score": null
    },
    "global_score": 93390.536
  },
  "raw_info": {
    "debug": "active",
    "dmidecode": "# dmidecode 3.6\nGetting SMBIOS data from sysfs.\nSMBIOS 3.3.0 present.\n\nHandle 0x0000, DMI type 0, 26 bytes\nBIOS Information\n\tVendor: American Megatrends International, LLC.\n\tVersion: F65e\n\tRelease Date: 09/20/2023\n\tAddress: 0xF0000\n\tRuntime Size: 64 kB\n\tROM Size: 16 MB\n\tCharacteristics:\n\t\tPCI is supported\n\t\tBIOS is upgradeable\n\t\tBIOS shadowing is allowed\n\t\tBoot from CD is supported\n\t\tSelectable boot is supported\n\t\tBIOS ROM is socketed\n\t\tEDD is supported\n\t\tJapanese floppy for NEC 9800 1.2 MB is supported (int 13h)\n\t\tJapanese floppy for Toshiba 1.2 MB is supported (int 13h)\n\t\t5.25\"/360 kB floppy services are supported (int 13h)\n\t\t5.25\"/1.2 MB floppy services are supported (int 13h)\n\t\t3.5\"/720 kB floppy services are supported (int 13h)\n\t\t3.5\"/2.88 MB floppy services are supported (int 13h)\n\t\tPrint screen service is supported (int 5h)\n\t\tSerial services are supported (int 14h)\n\t\tPrinter services are supported (int 17h)\n\t\tCGA/mono video services are supported (int 10h)\n\t\tUSB legacy is supported\n\t\tBIOS boot specification is supported\n\t\tTargeted content distribution is supported\n\t\tUEFI is supported\n\tBIOS Revision: 5.17\n\nHandle 0x0001, DMI type 1, 27 bytes\nSystem Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tUUID: 03c00218-044d-05b5-6506-740700080009\n\tWake-up Type: Power Switch\n\tSKU Number: Default string\n\tFamily: B450 MB\n\nHandle 0x0002, DMI type 2, 15 bytes\nBase Board Information\n\tManufacturer: Gigabyte Technology Co., Ltd.\n\tProduct Name: B450 AORUS ELITE\n\tVersion: Default string\n\tSerial Number: Default string\n\tAsset Tag: Default string\n\tFeatures:\n\t\tBoard is a hosting board\n\t\tBoard is replaceable\n\tLocation In Chassis: Default string\n\tChassis Handle: 0x0003\n\tType: Motherboard\n\tContained Object Handles: 0\n\nHandle 0x000B, DMI type 16, 23 bytes\nPhysical Memory Array\n\tLocation: System Board Or Motherboard\n\tUse: System Memory\n\tError Correction Type: None\n\tMaximum Capacity: 128 GB\n\tError Information Handle: 0x000A\n\tNumber Of Devices: 4\n\nHandle 0x0013, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0012\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0016, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0015\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL A\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C4408B\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x0019, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x0018\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 16 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 0\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: 00000000\n\tAsset Tag: Not Specified\n\tPart Number: CMW32GX4M2E3200C16  \n\tRank: 2\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: Unknown\n\tMaximum Voltage: Unknown\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 3, Hex 0x9E\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 16 GB\n\tCache Size: None\n\tLogical Size: None\n\nHandle 0x001C, DMI type 17, 92 bytes\nMemory Device\n\tArray Handle: 0x000B\n\tError Information Handle: 0x001B\n\tTotal Width: 64 bits\n\tData Width: 64 bits\n\tSize: 8 GB\n\tForm Factor: DIMM\n\tSet: None\n\tLocator: DIMM 1\n\tBank Locator: P0 CHANNEL B\n\tType: DDR4\n\tType Detail: Synchronous Unbuffered (Unregistered)\n\tSpeed: 3200 MT/s\n\tManufacturer: Unknown\n\tSerial Number: E3C44087\n\tAsset Tag: Not Specified\n\tPart Number: BL8G32C16U4BL.M8FE\n\tRank: 1\n\tConfigured Memory Speed: 3200 MT/s\n\tMinimum Voltage: 1.2 V\n\tMaximum Voltage: 1.2 V\n\tConfigured Voltage: 1.2 V\n\tMemory Technology: DRAM\n\tMemory Operating Mode Capability: Volatile memory\n\tFirmware Version: Unknown\n\tModule Manufacturer ID: Bank 6, Hex 0x9B\n\tModule Product ID: Unknown\n\tMemory Subsystem Controller Manufacturer ID: Unknown\n\tMemory Subsystem Controller Product ID: Unknown\n\tNon-Volatile Size: None\n\tVolatile Size: 8 GB\n\tCache Size: None\n\tLogical Size: None\n\n",
    "lsblk": "NAME        MAJ:MIN RM   SIZE RO TYPE MOUNTPOINTS\nloop0         7:0    0 118,5M  1 loop /snap/iptvnator/92\nloop1         7:1    0  48,1M  1 loop /snap/snapd/25935\nloop2         7:2    0  50,9M  1 loop /snap/snapd/25577\nloop3         7:3    0     4K  1 loop /snap/bare/5\nloop4         7:4    0  91,7M  1 loop /snap/gtk-common-themes/1535\nloop5         7:5    0  55,5M  1 loop /snap/core18/2976\nloop6         7:6    0 164,8M  1 loop /snap/gnome-3-28-1804/198\nloop7         7:7    0     0B  0 loop \nsda           8:0    0 447,1G  0 disk \n└─sda1        8:1    0 447,1G  0 part \nsdb           8:16   1     0B  0 disk \nsdc           8:32   1     0B  0 disk \nsdd           8:48   1     0B  0 disk \nsde           8:64   1     0B  0 disk \nnvme0n1     259:0    0 465,8G  0 disk \n├─nvme0n1p1 259:1    0   976M  0 part /boot/efi\n├─nvme0n1p2 259:2    0 440,8G  0 part /\n└─nvme0n1p3 259:3    0    24G  0 part [SWAP]\nnvme1n1     259:4    0 465,8G  0 disk \n├─nvme1n1p1 259:5    0    50M  0 part \n├─nvme1n1p2 259:6    0 464,3G  0 part \n├─nvme1n1p3 259:7    0   808M  0 part \n├─nvme1n1p4 259:8    0   100M  0 part \n└─nvme1n1p5 259:9    0   522M  0 part \n",
    "lscpu": "Architecture :                            x86_64\nMode(s) opératoire(s) des processeurs :   32-bit, 64-bit\nTailles des adresses:                     48 bits physical, 48 bits virtual\nBoutisme :                                Little Endian\nProcesseur(s) :                           24\nListe de processeur(s) en ligne :         0-23\nIdentifiant constructeur :                AuthenticAMD\nNom de modèle :                           AMD Ryzen 9 5900X 12-Core Processor\nFamille de processeur :                   25\nModèle :                                  33\nThread(s) par cœur :                      2\nCœur(s) par socket :                      12\nSocket(s) :                               1\nRévision :                                2\nAccroissement de fréquence :              activé\nmultiplication des MHz du/des CPU(s) :    96%\nVitesse maximale du processeur en MHz :   4951,0000\nVitesse minimale du processeur en MHz :   550,0000\nBogoMIPS :                                7399,98\nDrapeaux :                                fpu vme de pse tsc msr pae mce cx8 apic sep mtrr pge mca cmov pat pse36 clflush mmx fxsr sse sse2 ht syscall nx mmxext fxsr_opt pdpe1gb rdtscp lm constant_tsc rep_good nopl xtopology nonstop_tsc cpuid extd_apicid aperfmperf rapl pni pclmulqdq monitor ssse3 fma cx16 sse4_1 sse4_2 x2apic movbe popcnt aes xsave avx f16c rdrand lahf_lm cmp_legacy svm extapic cr8_legacy abm sse4a misalignsse 3dnowprefetch osvw ibs skinit wdt tce topoext perfctr_core perfctr_nb bpext perfctr_llc mwaitx cpb cat_l3 cdp_l3 hw_pstate ssbd mba ibrs ibpb stibp vmmcall fsgsbase bmi1 avx2 smep bmi2 erms invpcid cqm rdt_a rdseed adx smap clflushopt clwb sha_ni xsaveopt xsavec xgetbv1 xsaves cqm_llc cqm_occup_llc cqm_mbm_total cqm_mbm_local user_shstk clzero irperf xsaveerptr rdpru wbnoinvd arat npt lbrv svm_lock nrip_save tsc_scale vmcb_clean flushbyasid decodeassists pausefilter pfthreshold avic v_vmsave_vmload vgif v_spec_ctrl umip pku ospke vaes vpclmulqdq rdpid overflow_recov succor smca fsrm debug_swap\nVirtualisation :                          AMD-V\nCache L1d :                               384 KiB (12 instances)\nCache L1i :                               384 KiB (12 instances)\nCache L2 :                                6 MiB (12 instances)\nCache L3 :                                64 MiB (2 instances)\nNœud(s) NUMA :                            1\nNœud NUMA 0 de processeur(s) :            0-23\nVulnérabilité Gather data sampling :      Not affected\nVulnérabilité Indirect target selection : Not affected\nVulnérabilité Itlb multihit :             Not affected\nVulnérabilité L1tf :                      Not affected\nVulnérabilité Mds :                       Not affected\nVulnérabilité Meltdown :                  Not affected\nVulnérabilité Mmio stale data :           Not affected\nVulnérabilité Reg file data sampling :    Not affected\nVulnérabilité Retbleed :                  Not affected\nVulnérabilité Spec rstack overflow :      Mitigation; Safe RET\nVulnérabilité Spec store bypass :         Mitigation; Speculative Store Bypass disabled via prctl\nVulnérabilité Spectre v1 :                Mitigation; usercopy/swapgs barriers and __user pointer sanitization\nVulnérabilité Spectre v2 :                Mitigation; Retpolines; IBPB conditional; IBRS_FW; STIBP always-on; RSB filling; PBRSB-eIBRS Not affected; BHI Not affected\nVulnérabilité Srbds :                     Not affected\nVulnérabilité Tsa :                       Vulnerable: Clear CPU buffers attempted, no microcode\nVulnérabilité Tsx async abort :           Not affected\nVulnérabilité Vmscape :                   Mitigation; IBPB before exit to userspace\n"
  }
}
[DEBUG] Payload sauvegardé au format JSON dans bench_payload_last.json (49098 octets)
