######################################################################
## chaudiere
## actual value - input register
#   register_type: input
## FC=04 de 30001-30272   enlever 1 a register
######################################################################
- platform: modbus
  scan_interval: 10
  registers:
    - name: T° chaudiere
      hub: pimodbus
      register: 0
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 10
  registers:
    - name: T° fumée
      hub: pimodbus
      register: 1
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: T° board
      hub: pimodbus
      register: 2
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0

- platform: modbus
  scan_interval: 60
  registers:
    - name: T°exterieur nord
      device_class: temperature
      hub: pimodbus
      register: 4
      register_type: input
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: Ventilation
      hub: pimodbus
      register: 7
      register_type: input
      unit_of_measurement: U/min
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: Heure de chauffage
      hub: pimodbus
      register: 221
      register_type: input
      unit_of_measurement: h
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: Heure de service
      hub: pimodbus
      register: 98
      register_type: input
      unit_of_measurement: h
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 10
  registers:
    - name: T° départ
      hub: pimodbus
      register: 21
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 10
  registers:
    - name: Charge du tampon
      hub: pimodbus
      register: 225
      register_type: input
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 10
  registers:
    - name: tampon haut
      hub: pimodbus
      register: 118
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 10
  registers:
    - name: tampon bas
      hub: pimodbus
      register: 120
      register_type: input
      device_class: temperature
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 0.5
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: Consigne T° fumée
      device_class: temperature
      hub: pimodbus
      register: 19
      register_type: input
      unit_of_measurement: °C
      slave: 2
      count: 1
      scale: 1
      offset: 0
      precision: 0
- platform: modbus
  scan_interval: 60
  registers:
    - name: Etat chaudiere
      hub: pimodbus
      register: 4001
      register_type: input
      slave: 2
      count: 1
      scale: 1
- platform: modbus
  scan_interval: 60
  registers:
    - name: O2_residuel
      hub: pimodbus
      register: 3
      register_type: input
      slave: 2
      count: 1
      scale: 0.1
      offset: 0
      precision: 0
######################################################################
## chaudiere
## parameter - holding registers
#  register_type: holding
## FC=03 de 40001-41094   enlever 1 a register
######################################################################