######################################################################
## chaudiere
## actual value - input register
#   register_type: input
## FC=04 de 30001-30272   enlever 1 a register
######################################################################

- unique_id: temp_chaud_01
  state_topic: "chaudiere/t_chaud"
  unit_of_measurement: "°C"
  device_class: temperature
  name: "T° chaudiere"
- unique_id: temp_fumee_01
  state_topic: "chaudiere/t_fumee"
  name: "T° fumée"
  device_class: temperature
  unit_of_measurement: "°C"
- unique_id: temp_board_01
  state_topic: "chaudiere/t_board"
  name: "T° board"
  device_class: temperature
  unit_of_measurement: "°C"

- unique_id: temp_ext_N_01
  state_topic: "chaudiere/t_ext"
  name: "T°exterieur nord"
  device_class: temperature
  unit_of_measurement: "°C"
  

- unique_id: venti_chaud_01
  state_topic: "chaudiere/vit_venti"
  name: "Ventilation"
  unit_of_measurement: "U/min"
  

- unique_id: heure_chauff_01
  state_topic: "chaudiere/h_chauffage"
  name: "Heure de chauffage"
  unit_of_measurement: "h"
  

- unique_id: heure_serv_01
  state_topic: "chaudiere/h_service"
  name: "Heure de service"
  unit_of_measurement: "h"
  

- unique_id: temp_dep_chauff_01
  state_topic: "chaudiere/t_dep_chauff"
  name: "T° départ"
  device_class: temperature
  unit_of_measurement: "°C"
  

- unique_id: charge_tampon_01
  state_topic: "chaudiere/charge_tampon"
  name: "Charge du tampon"
  

- unique_id: tampon_haut_01
  state_topic: "chaudiere/tampon_haut"
  name: "tampon haut"
  device_class: temperature
  unit_of_measurement: "°C"
  

- unique_id: tampon_bas_01
  state_topic: "chaudiere/tampon_bas"
  name: "tampon bas"
  device_class: temperature
  unit_of_measurement: "°C"
  

- unique_id: temp_cons_fumee_01
  state_topic: "chaudiere/cons_t_fumee"
  name: "Consigne T° fumée"
  device_class: temperature
  unit_of_measurement: "°C"
  

- unique_id: etat_chaud_01
  state_topic: "chaudiere/etat_chaudiere"
  name: "Etat chaudiere"
  

- unique_id: O2_resi_01
  state_topic: "chaudiere/O2_res"
  name: "O2_residuel"
  
######################################################################
## chaudiere
## parameter - holding registers
#  register_type: holding
## FC=03 de 40001-41094   enlever 1 a register
######################################################################

